Below you can find a screenshot of the Pure Data patch, aimed to let you quickly understand how it works.

Please refer to the following colour legend to have a grasp of the features;

* red = F0 and harmonics frequencies, as F0 multipliers
* green = partials amplitudes
* blue = calculated harmonicity
* violet = calculated spectral centroid
* black = output file name
* brown = start recording